A case for storing the tiles of Rallyman GT
by ikegami@adaelis.com

This project consists of the design for a laser-cut
case for storing the tiles of Rallyman GT.

The design is large enough to accommodate all
the tiles from the following products combined:
- The base game
- Kickstarter exclusives
- Championship
- World Tour
- Team Challenge

Designed for 0.12" thick material (e.g. 1/8" hardboard).
A tiny amount of 1/4" thick material is also needed.
(One shouldn't use two 1/8" pieces glued together for the shaft.)

Cut along the magenta lines for an 0.005" undercut (for a tight fit).

No adhesive or fasteners are needed except where indicated by the following:
- The latch, shaft, spacer and knob pieces must be glued together.
- The optional nameplate must be glued on.
- You may optionally glue the outer and inner end pieces together.

The edges the sides will need to be sanded down to an angle.
This is very easy to do with a belt sander. Alternatively,
you may reduce the width of the side pieces.

Possible improvements:
- Add a loop to the top of the "Outer End Top" pieces to add
  a carrying strap or handle.

Feel free to reach out to me for comments or help.
ikegami@adaelis.com
